EXHIBIT 1


ZONE 16 IMPROVEMENTS TO BE MAINTAINED


Certain public storm drainage improvements are to be installed by the developers as part of the Conditions of Approval for the Tra Vigne West Project. Tra Vigne West Project Zone 16 was created to fund the continued maintenance of the storm drainage facilities described below.  During the construction period of each phase, the developer will maintain the drainage improvements until June 30th of the following year, at which time the new improvements within the recorded unit shall be incorporated into Tra Vigne West Zone 16 of the Assessment District. 

The following improvements shall be included in Zone 16 upon their completion: 

1. A Contech CDS5678-10-C771343-10 Hydrodynamic Separator, to be maintained per manufacturer's recommendations. 

2. The inlet and outlet structures for the basin to be inspected and maintained as needed. 

3. The storm pump station, which discharges into Bear Creek, is to be inspected and maintained annually. 

4. The generator yard, at the pump station, is to be inspected and maintained annually.

5. The Bear Creek Outfall is to be inspected and maintained as needed. 

6. A detention basin to be maintained and inspected periodically for: slope stability, sediment accumulation, trash and debris, presence of burrows, and mowless grass or approved equivalent. 

7. Vector control to be inspected and treated. 

8. The wrought iron fence (~3,100 LF) and two gates that surround the extended detention basin are to be inspected and maintained. 

9. An asphalt concrete access road to be maintained.
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